Cen- Stat

The cen-state range of clamps, cables, reels are single circuit applications that rely on high strength of mechanical circuits to dissipate static electricity from potentially charged equipment

Cen- state clamps are specially designed to dissipate static electricity from potentially charged equipment and subjected to FM and ATEX testing standards.

In many cases, hazardous are operators, rely on small clips and welding clamps to ground the equipment without any guarantee that they are penetrating hardened product deposits, or rust or paint. To diminish the uncertainty of connection, Cen-stat clamps are fitted with pair of tungsten carbide tips to bit through the connection inhibitors and achieve the direct electrical contact to potentially charged equipment. The stainless steel construction of the clamps provides corrosion resistant benefit and capable of working through industrial environment

The earthing clamp is being supplied with static dissipative hytrel coated spiral cables or static discharge variety of reels.

**Products**

|  |  |
| --- | --- |
| X90 & 45 clamp photo |  |
| Cable photos- bunch of green, blue and organge |  |
| Yellow cable reels |  |
| Hand wound reels |  |
| Multi meter |  |
| Sole mat |  |
| Quick connectors |  |